Net2 - Reconnect Door Controllers


Open - Net2 Configuration Utility

A close-up of a sign

Description automatically generated

Login using system engineer

Click **TCP/IP Nodes**



Click **Detect** then click **Apply** then click **OK**

A screenshot of a computer

Description automatically generated

Click **Yes** to restart Server  
A screenshot of a computer

Description automatically generated

Now Open Net2 Software and login  
  
Click **Doors**  
  
A screenshot of a computer

Description automatically generated

Doors should show the **Green Tick**